**Public Address System 10 Channel Monitor Panel
FY-10MP**

**FEATURES:**

* Public address system monitor panel.
* Design with 10 channel inputs.
* Built-in monitor speaker to listen and monitor the system output.
* The monitor speaker with adjustable volume control.
* A five-element LED level meter is provided.

**SPECIFICATIONS:**

|  |  |
| --- | --- |
| **Model** | **FY-10MP** |
| **Description** | **10 Channel Monitor Panel** |
| Inputs | 70-100V , 10kΩ |
| Output | 65dB SPL Variable |
| Frequency response | 100Hz-15kHz |
| Signal to noise ratio | 80dB |
| Speak | Inside |
| Protection | AC fuse |
| Power Requirement | AC 220-240V/50-60Hz |
| Outer Packing Size (mm) | (L×W×H)530×440×195 |
| Unit Size (mm) | (L×W×H)484×365×88 |
| Gross weight | 8.2kg |
| Net weight | 6.5kg |