**Telephone Paging Interface
FY-206T**
**Features:**

* Main equipment to make remote telephone paging over the public address system.
* 19” rack mount design with mounting handles.
* Automatic and manual phone call answer selection buttons on front panel.
* Automatic hang up after paging.
* Telephone conversation function is available.
* Ring bell times pre-setting available.
* Short-circuited signal output for system activation after phone call come in.
* Built-in 5W/8Ω monitor speaker.
* Separate monitor and output volume control.
* With one contact input, one telephone input, one microphone input and one aux output.
* Work with versatile PABX system for telephone paging system.

**Specifications:**

|  |  |
| --- | --- |
| **Model** | **FY-206T** |
| **Description** | **Telephone Paging Interface** |
| **Connectors** | One close contact by 6.3mm Jack, 0VTelephone input by RJ-11One Microphone input by 6.3mm JackOne Aux output by RCA, 10KΩ, 200mV-0.775V (0dB) |
| **Control** | Manual/Auto answer selection buttonSeparate monitor & output volume control |
| **Monitor Speaker** | 5W, 8Ω, full range |
| **Power Consumption** | 10W |
| **Power Supply** | 230V AC, 50-60Hz |
| **Dimension** | 484(W)×88(H)×350(D)mm |
| **Accessory** | RJ-11 cable, 1.5 meters,  AC power cord |