**Voice Evacuation & Fire Alarm Panel with Recorder**

**FY-200E**

**FEATURES:**

* Automatically broadcast voice alarm message after trigger by fire system.
* Built-in voice recorder and fire alarm generator.
* The recorder available through external microphone and external line.
* The recorder with start, stop and play functions.
* The system with siren, play, record and off selective knob.
* One voice alarm input and one alarm output by phone jack type.
* One microphone input and one line input by phone jack type
* 1 minute of digital customized voice evacuation message to the built-in memory IC.
* With record volume and alarm output volume attenuator by protective knobs.
* With Fire, start, stop and power working status indicators.

**SPECIFICATIONS:**

|  |  |
| --- | --- |
| **Model** | FY-200E |
| **Name** | **Voice Evacuation & Fire Alarm Panel with Recorder** |
| **Inputs** | Microphone: <5mV, 600Ω, unbalanced;   Line: <400mV 10kΩ, unbalanced; |
| Output | >200mV Sire or Recorded Message |
| Recorder | IC inside, 60 seconds, write in more than 8,000 times. |
| Frequency Response | 100Hz-3.4kHz（±3dB） |
| Alarm Input | One alarm input, 0V short circuit closed contact |
| Power Requirement | AC 220-240V/50-60Hz |
| Dimension | 484(W)×350(D)×88(H)mm |
| Packaging | 520(W)×435(D)×185(H)mm |
| Net Weight | 6.1kg |
| Gross Weight | 7.8kg |