**4.5" Frameless Ceiling Speaker (3W-6W)
FCS-705N**

****

**Feature:**

* Commercial ceiling speaker with transformer.
* 4.5” ceiling speaker for BGM and PA system use.
* Compact size consistent with spot lighting and architectural design.
* Ideal for school, office, hotel and airport background music system.
* Rated power output 3W-6W at 100V.
* 5" full range paper driver unit.
* Line input 100V or 70V.
* ABS enclosure and metal grille in white.
* In-ceiling quick installation by spring clip.

**Specification:**

|  |  |
| --- | --- |
| **Model** | **FCS-705N** |
| **Description** | 4.5” Ceiling Speaker  |
| **Rated Power Output** | 3W-6W |
| **Line Input** | 100V or 70V |
| **Frequency Response** | 120Hz-18KHz |
| **SPL(@1W/m)** | 92dB ±3db |
| **Speaker Unit** | 4.5” full range paper cone |
| **Cutout Size** | 148mm |
| **Dimension** | 160D)×56(H)mm |
| **Material** | ABS enclosure and metal grille in white |
| **Mounting Way** | In-ceiling spring clip quick installation |
| **Weight** | 0.42kg |

**Frequency Response VS SPL:**

****